**Driver Vehicle Inspection Report (DVIR)**

Driver First Name: Driver Last Name:



**DSP Code & Company Name:** ORMP-ONRAMP

Vehicle Identification Number (VIN):

License Plate:

License Plate State: FL

Asset type: Current Odometer Reading:

Inspection Location Station Code: HTP1

I**nspection Date (MM/DD/YYYY): Start Time: AM / PM** (circle one) **Inspection Type: Pre-Trip / Post-Trip** (circle one)

Check **(√)** any defective item needing repairs, replacement or affecting normal operations.

\* = OUT OF SERVICE DEFECT THAT MUST GROUND THE VEHICLE IMMEDIATELY UNTIL THE SAFETY ISSUE IS FIXED

|  |  |  |
| --- | --- | --- |
| **1. FRONT SIDE OF VEHICLE** | | |
| **Parts and Accessories** | **Defects** | **√** |
| Lights and light covers | \*Lights or light covers are cracked, broken, or missing |  |
| \*Headlight is not working |  |
| \*Hazard light is not working |  |
| Suspension & exhaust System | \*Loose or hanging objects underneath |  |
| \*Noticeable leaning of vehicle (when parked) |  |
| Electric Vehicle (EV) system | \*Battery boxes are unsecured or damaged |  |
| \*Any loose, hanging, faulty, or frayed wires |  |
| \*Orange wires are present: High Voltage! Do not touch! |  |
| **2. PASSENGER SIDE** | | |
| Side mirrors | \*Mirror or glass is missing |  |
| Bulb cover is missing |  |
| Plastic casing is missing, or broken |  |
| \*Side mirrors have cracks or damage but is not in your line of sight |  |
| \*Side mirrors have cracks or damage that is in your line of sight |  |
| \*Side mirrors are loose, hanging, unsecured, or held up with a zip-tie, tape, or similar |  |
| Side mirrors cannot be adjusted |  |
| Front tire, wheel and rim | \*Tire is flat, leaking air, bulging, or swelling |  |
| \*Tire has objects, cuts, dents, or exposed wire on its surface |  |
| \*Tire has insufficient tread (Less than 2/32" or 1.6mm) |  |
| \*Tire has insufficient tread (Less than 4/32" or 3.2mm) |  |
| \*Tire has uneven wear on treads |  |
| \*Wheel, rim, or mounting equipment is damaged, cracked, or broken |  |
| \*Wheel nuts are missing, or loose |  |
| Fuel and fluids | Fuel cap is missing or broken |  |
| \*Charging port cap is missing or broken |  |
| \*Active red, orange, yellow, green, blue, brown, black, or pink fluid leaking on the ground |  |
| Lights and light covers | \*Lights or light covers are cracked, broken, or missing |  |
| Body and doors | Scratch/dent/chips that are more than 6 inches (15 cm) |  |
| Punctured holes, or sharp edges |  |
| \*Items attached to the body of the vehicle (for example: bumper, lift gates, back and cargo steps) are missing,  damaged, loose, unsecure, hanging, or held with a zip-tie, tape, or similar |  |
| \*Doors cannot open, or close |  |
| Doors cannot lock correctly |  |
| Other |  |
| Suspension & exhaust system | \*Loose or hanging objects underneath |  |
| \*Noticeable leaning of vehicle (when parked) |  |
| EV system | \*Battery boxes are unsecured or damaged |  |
| \*Any loose, hanging, faulty, or frayed wires |  |
| \*Orange wires are present: High Voltage! Do not touch! |  |
| Back tire, wheel and rim | \*Tire is flat, leaking air, bulging, or swelling |  |
| \*Tire has objects, cuts, dents, or exposed wire on its surface |  |
| \*Tire has insufficient tread (Less than 2/32" or 1.6mm) |  |

|  |  |  |
| --- | --- | --- |
|  | \*Tire has uneven wear on treads |  |
| \*Wheel, rim, or mounting equipment is damaged, cracked, or broken |  |
| \*Wheel nuts are missing, or loose |  |
| **3. BACK SIDE** | | |
| Camera/monitor | \*Back-up camera is loose, hanging, missing, or mounted with a tape, zip-tie, or similar |  |
| Lights and light covers | \*Lights or light covers are cracked, broken, or missing |  |
| \*Tail light is not working |  |
| \*Hazard light is not working |  |
| \*License plate light is not working |  |
| Body and doors | Scratch/dent/chips that are more than 6 inches (15 cm) |  |
| Punctured holes, or sharp edges |  |
| \*Items attached to the body of the vehicle (for example: bumper, lift gates, back and cargo steps) are missing,  damaged, loose, unsecure, hanging, or held with a zip-tie, tape, or similar |  |
| \*Doors cannot open, or close |  |
| Doors cannot lock correctly |  |
| Other |  |
| License plates/tags | \*License plates/temp tags/ are damaged, missing, or expired |  |
| \*DOT/CA BIT/ State Inspection sticker is missing or expired |  |
| Suspension & exhaust system | \*Loose or hanging objects underneath |  |
| \*Noticeable leaning of vehicle (when parked) |  |
| EV system | \*Battery boxes are unsecured or damaged |  |
| \*Any loose, hanging, faulty, or frayed wires |  |
| \*Orange wires are present: High Voltage! Do not touch! |  |
| **4. DRIVER SIDE** | | |
| Back tire, wheel and rim | \*Tire is flat, leaking air, bulging, or swelling |  |
| \*Tire has objects, cuts, dents, or exposed wire on its surface |  |
| \*Tire has insufficient tread (Less than 2/32" or 1.6mm) |  |
| \*Tire has uneven wear on treads |  |
| \*Wheel, rim, or mounting equipment is damaged, cracked, or broken |  |
| \*Wheel nuts are missing, or loose |  |
| Fuel and fluids | Fuel cap is missing or broken |  |
| \*Charging port cap is missing or broken |  |
| \*Active red, orange, yellow, green, blue, brown, black, or pink fluid leaking on the ground |  |
| Lights and light covers | \*Lights or light covers are cracked, broken, or missing |  |
| Body and doors | Scratch/dent/chips that are more than 6 inches (15 cm) |  |
| Punctured holes, or sharp edges |  |
| \*Items attached to the body of the vehicle (for example: bumper, lift gates, back and cargo steps) are missing,  damaged, loose, unsecure, hanging, or held with a zip-tie, tape, or similar |  |
| \*Doors cannot open, or close |  |
| Doors cannot lock correctly |  |
| Other |  |
| Suspension & exhaust system | \*Loose or hanging objects underneath |  |
| \*Noticeable leaning of vehicle (when parked) |  |
| EV system | \*Battery boxes are unsecured or damaged |  |
| \*Any loose, hanging, faulty, or frayed wires |  |
| \*Orange wires are present: High Voltage! Do not touch! |  |
| Side mirrors | \*Mirror or glass is missing |  |
| Bulb cover is missing |  |
| Plastic casing is missing, or broken |  |
| Side mirrors have cracks or damage but is not in your line of sight |  |
| \*Side mirrors have cracks or damage that is in your line of sight |  |
| \*Side mirrors are loose, hanging, unsecured, or held up with a zip-tie, tape, or similar |  |
| Side mirrors cannot be adjusted |  |
| Front tire, wheel and rim | \*Tire is flat, leaking air, bulging, or swelling |  |
| \*Tire has objects, cuts, dents, or exposed wire on its surface |  |

|  |  |  |
| --- | --- | --- |
|  | \*Tire has insufficient tread (Less than 2/32" or 1.6mm) |  |
| \*Tire has insufficient tread (Less than 4/32" or 3.2mm) |  |
| \*Tire has uneven wear on treads |  |
| \*Wheel, rim, or mounting equipment is damaged, cracked, or broken |  |
| \*Wheel nuts are missing, or loose |  |
| **5. IN CAB** | | |
| Steering, seatbelt, horn, and alarm | \*Steering wheel has excessive vibration |  |
| Steering wheel is stiff, loose, or needs alignment |  |
| \*Seatbelt is missing, torn, or frayed |  |
| \*Seatbelt is not working |  |
| \* Horn, backup alarm, or seatbelt alarm is not working |  |
| Wipers | \*Wipers are missing, damaged, or not working |  |
| \*Windshield washer system/wiper fluid reservoir is not working |  |
| \*Defroster/heater is not working |  |
| Windshield | Windshield has crack/chips/stars/bullseyes or damage but it is not in your line of sight |  |
| \*Windshield has crack/chips/stars/bullseyes or damage that is in your line of sight |  |
| \*Windshield has crack/chips/stars/bullseyes or damage that is more than 1 inch |  |
| \*Device/Accessory is mounted on the windshield |  |
| HVAC systems | \*Defroster/heater is not working |  |
| \*Low air flow from vents |  |
| AC not blowing cold air |  |
| Dashboard warning light | \*Any red warning lights/lamps are on or flashing |  |
| \*State of charge is low (< 95%) |  |
| Brakes | \* Air pressure gauge read less than 79 lb./in2 (5.5 kg/cm2) |  |
| Foot brake is squeaking |  |
| \*Foot brake has leaking air |  |
| \*Foot brake vibrates |  |
| \*Foot brake is grinding, or not working |  |
| Foot brake is loose, or stiff |  |
| \*Parking brake is not working |  |
| Parking brake is loose, weak, or stiff |  |
| \*Parking brake is engaged and dashboard light is not on |  |
| \*Parking brake is not engaged and dashboard light is on |  |
| Lights and light covers | \*Turn signal is not working |  |
| \*Hazard light is not working |  |
| \*Dashboard light is not working |  |
| Safety accessories | \*Fire extinguisher is missing, mounted with a tape, zip-tie or similar, or the dial/needle is not in the green zone |  |
| \*Delivery device cradle is damaged, missing, or is mounted with a tape, zip-tie or similar |  |
| \*Reflective triangles are missing |  |
| \*Spare fuses are missing |  |
| Camera/monitor | \*Camera monitor is missing, broken, or not working |  |
| \*Camera monitor is mounted with a tape, zip-tie, or similar |  |
| \*Back-up camera is loose, hanging, missing, or mounted with a tape, zip-tie, or similar |  |
| \*Netradyne camera is hanging/disconnected from bracket |  |
| Vehicle documentation | \*Insurance Information is missing or expired |  |
| \*Short Haul Exemption is missing or expired |  |
| \*Vehicle Registration is missing or expired |  |
| \*Certification of Lease is missing |  |
| Vehicle Cleanliness | Exterior of vehicle is visibly dirty when viewed from 20 feet away |  |
| Amazon Prime decal is damaged, missing, or excessively dirty |  |
| Interior of vehicle has excessive grime, dust, or trash present |  |

* VEHICLE IS IN SATISFACTORY CONDITION

X

DRIVER’S SIGNATURE UPON COMPLETION OF ABOVE CHECKLIST

* ABOVE DEFECTS HAVE BEEN CORRECTED
* ABOVE DEFECTS DO NOT NEED TO BE CORRECTED FOR SAFE OPERATION OF THE VEHICLE

MECHANIC’S SIGNATURE DATE: DRIVER’S SIGNATURE DATE: